[MountMonitor Version]
(v.3.37 210103)
[E-Mail]
nicolas@dehilster.info
[Mount name]
10micron GM3000HPS
[Site name]
My Observatory
[ASCOM driver]

[IP address]
10.0.1.151
[Port]
3492
[Command mode]
0
[Delay after slewing mode]
0
[Polling mode]
0
[Logging mode]
1
[Tolerance RA/DEC mode]
5
[Use as HA tolerance]
false
[Axis speed mode index]
3
[Show Seismometer Data]
false
[Seismometer Serial Port]
0
[Tolerance Seismometer Mode]
0
[Seismometer Offset]
300
[Seismometer Range]
2000
[NIST Time Server]
time-a-g.nist.gov
[Use NIST Time Server]
true
[NIST Time Polling Interval]
1
[Time Graph Max Zoom-out Value]
0
[Running range mode]
0
[Adjust Graphs For Running Range Length]
true
[Reference mode]
0
[Horizontal Zoom mode]
4
[Vertical Zoom mode]
2
[Reset buffers and min/max mode]
1
[Dump graphs mode]
2
[Close files mode]
2
[Frame Width (px)]
1459
[Frame Height (px)]
842
[Frame X (px)]
159
[Frame Y (px)]
24
[Graph to Textbox Ratio (textbox = 1)]
3
[FFT Box Width (px)]
930
[FFT Box Height (px)]
426
[FFT Box X (px)]
100
[FFT Box Y (px)]
100
[Checks to be performed]
23~1~1
24~2~1
25~0~1
26~1~1
27~0~1
[/Checks to be performed]
